## APPENDIX P: Place LHD Logo Here

## Respirator Storage, Cleaning, Maintenance and Repair

Our non-disposable respirators will be stored in the following clean locations:

Respirators will be cleaned and sanitized every (\_\_\_\_\_) days or whenever they are visibly dirty. This does not apply to paper dust masks which are disposed daily. Respirators will be cleaned according to the attached instructions (either the manufacturer’s instructions or the Respirators Rule cleaning procedures).

For Rule-specified respirator cleaning procedures where you don’t have manufacturer’s instructions, see below.

* All respirators will be inspected before and after every use and during cleaning. In addition, emergency respirators and self-contained tank-type supplied air respirators in storage will be inspected monthly.
* Respirators will be inspected for damage, deterioration or improper functioning and repaired or replaced as needed. Repairs and adjustments are done by \_\_\_\_\_\_\_\_\_\_\_\_ who is trained in respirator maintenance and repair.
* Supplied air respirators will be checked for proper functioning of regulator and warning devices and amount of air in tanks where used.
* When supplied air respirators are used, any needed repairs or adjustments will be done by the manufacturer or technician trained by the manufacturer. Our supplied air respirators are maintained and repaired by \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.
* On respirators with vapor or gas cartridges, the cartridges will be regularly replaced on the following schedule. Check with respirator vendor for recommended replacement schedule for each brand and type of respirator.

|  |  |  |  |
| --- | --- | --- | --- |
| **Type of respirator cartridge** | **Location or job duties** | **Chemicals in use** | **Replacement schedule** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**PHPS-R005**

**7/1/2018**